\documentclass[format=acmsmall, review=false]{acmart}
\usepackage{acm-ec-22}
\usepackage{booktabs} % For formal tables
\usepackage[ruled]{algorithm2e} % For algorithms
\renewcommand{\algorithmcfname}{ALGORITHM}
\SetAlFnt{\small}
\SetAlCapFnt{\small}
\SetAlCapNameFnt{\small}
\SetAlCapHSkip{0pt}
\IncMargin{-\parindent}

% Choose a citation style by commenting/uncommenting the appropriate line:
%\setcitestyle{acmnumeric}
\setcitestyle{authoryear}

% Title. Note the optional short title for running heads. In the interest of anonymization, please do not include any acknowledgements.
\title[A VCG-Based Mechanism for Electronic Commerce]{A VCG-Based Mechanism for Electronic Commerce Applications}

% Anonymized submission.
\author{Submission 42}

% Abstract. Note that this must come before \maketitle.
\begin{abstract}
In auction theory, a Vickrey--Clarke--Groves (VCG) auction is a type of sealed-bid auction of multiple items. Bidders submit bids that report their valuations for the items, without knowing the bids of the other people in the auction. The auction system assigns the items in a socially optimal manner: it charges each individual the harm they cause to other bidders. It also gives bidders an incentive to bid their true valuations, by ensuring that the optimal strategy for each bidder is to bid their true valuations of the items. (Thanks for this text, Wikipedia.) This paper shows that the same idea works for electronic commerce applications.
\end{abstract}

\begin{document}

% Title page for title and abstract only.
\begin{titlepage}

\maketitle

\end{titlepage}

% Paper body
\section{Introduction}

Since we're all intimately familiar with VCG, let's learn about Wireless Sensor Networks by using the standard ACM demo article text from here on.

As a new technology, Wireless Sensor Networks (WSNs) has a wide
range of applications \cite{Culler-01, Bahl-02, Akyildiz-01}, including
environment monitoring, smart buildings, medical care, industrial and
military applications. Among them, a recent trend is to develop
commercial sensor networks that require pervasive sensing of both
environment and human beings, for example, assisted living
\cite{Akyildiz-02, Harvard-01,CROSSBOW} and smart homes
\cite{Harvard-01, Adya-01,CROSSBOW}.
% quote
\begin{quote}
	``For these applications, sensor devices are incorporated into human
	cloths \cite{Natarajan-01, Zhou-06, Bahl-02, Adya-01} for monitoring
	health related information like EKG readings, fall detection, and
	voice recognition''.
\end{quote}
While collecting all these multimedia information
\cite{Akyildiz-02} requires a high network throughput, off-the-shelf
sensor devices only provide very limited bandwidth in a single
channel: 19.2\,Kbps in MICA2 \cite{Bahl-02} and 250\,Kbps in MICAz.

In this article, we propose MMSN, abbreviation for Multifrequency
Media access control for wireless Sensor Networks. The main
contributions of this work can be summarized as follows.
% itemize
\begin{itemize}
	\item To the best of our knowledge, the MMSN protocol is the first
	multifrequency MAC protocol especially designed for WSNs, in which
	each device is equipped with a single radio transceiver and
	the MAC layer packet size is very small.
	\item Instead of using pairwise RTS/CTS frequency negotiation
	\cite{Adya-01, Culler-01, Tzamaloukas-01, Zhou-06},
	we propose lightweight frequency assignments, which are good choices
	for many deployed comparatively static WSNs.
	\item We develop new toggle transmission and snooping techniques to
	enable a single radio transceiver in a sensor device to achieve
	scalable performance, avoiding the nonscalable ``one
	control channel + multiple data channels'' design \cite{Natarajan-01}.
\end{itemize}

% Head 1
\section{MMSN Protocol}

% Head 2
\subsection{Frequency Assignment}

We propose a suboptimal distribution to be used by each node, which is
easy to compute and does not depend on the number of competing
nodes. A natural candidate is an increasing geometric sequence, in
which
% Numbered Equation
\begin{equation}
\label{eqn:01}
P(t)=\frac{b^{\frac{t+1}{T+1}}-b^{\frac{t}{T+1}}}{b-1},
\end{equation}
where $t=0,{\ldots}\,,T$, and $b$ is a number greater than $1$.

In our algorithm, we use the suboptimal approach for simplicity and
generality. We need to make the distribution of the selected back-off
time slice at each node conform to what is shown in
Equation~\eqref{eqn:01}. It is implemented as follows: First, a random
variable $\alpha$ with a uniform distribution within the interval $(0,
1)$ is generated on each node, then time slice $i$ is selected
according to the following equation:
% Unnumbered Equation
\[
i=\lfloor(T+1)\log_b[\alpha(b-1)+1]\rfloor.
\]
It can be easily proven that the distribution of $i$ conforms to Equation
(\ref{eqn:01}).

So protocols \cite{Bahl-02, Culler-01,Zhou-06,Adya-01,
	Tzamaloukas-01, Akyildiz-01} that use RTS/CTS
controls\footnote{RTS/CTS controls are required to be implemented by
	802.11-compliant devices. They can be used as an optional mechanism
	to avoid Hidden Terminal Problems in the 802.11 standard and
	protocols based on those similar to \citet{Akyildiz-01} and
	\citet{Adya-01}.} for frequency negotiation and reservation are not
suitable for WSN applications, even though they exhibit good
performance in general wireless ad hoc
networks.

% Head 3
\subsubsection{Exclusive Frequency Assignment}


In exclusive frequency assignment, nodes first exchange their IDs
among two communication hops so that each node knows its two-hop
neighbors' IDs. In the second broadcast, each node beacons all
neighbors' IDs it has collected during the first broadcast period.

% Head 4
\paragraph{Eavesdropping}

Even though the even selection scheme leads to even sharing of
available frequencies among any two-hop neighborhood, it involves a
number of two-hop broadcasts. To reduce the communication cost, we
propose a lightweight eavesdropping scheme.

\subsection{Basic Notations}

As Algorithm~\ref{alg:one} states, for each frequency
number, each node calculates a random number (${\textit{Rnd}}_{\alpha}$) for
itself and a random number (${\textit{Rnd}}_{\beta}$) for each of its two-hop
neighbors with the same pseudorandom number generator.

% Algorithm
\begin{algorithm}[t]
	\SetAlgoNoLine
	\KwIn{Node $\alpha$'s ID ($ID_{\alpha}$), and node $\alpha$'s
		neighbors' IDs within two communication hops.}
	\KwOut{The frequency number ($FreNum_{\alpha}$) node $\alpha$ gets assigned.}
	$index$ = 0; $FreNum_{\alpha}$ = -1\;
	\Repeat{$FreNum_{\alpha} > -1$}{
		$Rnd_{\alpha}$ = Random($ID_{\alpha}$, $index$)\;
		$Found$ = $TRUE$\;
		\For{each node $\beta$ in $\alpha$'s two communication hops
		}{
			$Rnd_{\beta}$ = Random($ID_{\beta}$, $index$)\;
			\If{($Rnd_{\alpha} < Rnd_{\beta}$) \text{or} ($Rnd_{\alpha}$ ==
				$Rnd_{\beta}$ \text{and} $ID_{\alpha} < ID_{\beta}$)\;
			}{
				$Found$ = $FALSE$; break\;
			}
		}
		\eIf{$Found$}{
			$FreNum_{\alpha}$ = $index$\;
		}{
			$index$ ++\;
		}
	}
	\caption{Frequency Number Computation}
	\label{alg:one}
\end{algorithm}


Bus masters are divided into two disjoint sets, $\mathcal{M}_{RT}$
and $\mathcal{M}_{NRT}$.
% description
\begin{description}
	\item[RT Masters]
	$\mathcal{M}_{RT}=\{ \vec{m}_{1},\dots,\vec{m}_{n}\}$ denotes the
	$n$ RT masters issuing real-time constrained requests. To model the
	current request issued by an $\vec{m}_{i}$ in $\mathcal{M}_{RT}$,
	three parameters---the recurrence time $(r_i)$, the service cycle
	$(c_i)$, and the relative deadline $(d_i)$---are used, with their
	relationships.
	\item[NRT Masters]
	$\mathcal{M}_{NRT}=\{ \vec{m}_{n+1},\dots,\vec{m}_{n+m}\}$ is a set
	of $m$ masters issuing nonreal-time constrained requests. In our
	model, each $\vec{m}_{j}$ in $\mathcal{M}_{NRT}$ needs only one
	parameter, the service cycle, to model the current request it
	issues.
\end{description}

Here, a question may arise, since each node has a global ID. Why
don't we just map nodes' IDs within two hops into a group of
frequency numbers and assign those numbers to all nodes within two
hops?

\section{Simulator}
\label{sec:sim}

If the model checker requests successors of a state which are not
created yet, the state space uses the simulator to create the
successors on-the-fly. To create successor states the simulator
conducts the following steps.
% enumerate
\begin{enumerate}
	\item Load state into microcontroller model.
	\item Determine assignments needed for resolving nondeterminism.
	\item For each assignment.
	\begin{enumerate}
		\item either call interrupt handler or simulate effect of next instruction, or
		\item evaluate truth values of atomic propositions.
	\end{enumerate}
	\item Return resulting states.
\end{enumerate}
Figure~\ref{fig:one} shows a typical microcontroller C program that
controls an automotive power window lift. The program is one of the
programs used in the case study described in Section~\ref{sec:sim}.
At first sight, the programs looks like an ANSI~C program. It
contains function calls, assignments, if clauses, and while loops.
% Figure
\begin{figure}
	\includegraphics{mouse}
	\caption{Code before preprocessing.}
	\label{fig:one}
\end{figure}

\subsection{Problem Formulation}

The objective of variable coalescence-based offset assignment is to find
both the coalescence scheme and the MWPC on the coalesced graph. We start
with a few definitions and lemmas for variable coalescence.

% Enunciations
\begin{definition}[Coalesced Node (C-Node)]A C-node is a set of
	live ranges (webs) in the AG or IG that are coalesced. Nodes within the same
	C-node cannot interfere with each other on the IG. Before any coalescing is
	done, each live range is a C-node by itself.
\end{definition}

\begin{definition}[C-AG (Coalesced Access Graph)]The C-AG is the access
	graph after node coalescence, which is composed of all C-nodes and C-edges.
\end{definition}

\begin{lemma}
	The C-MWPC problem is NP-complete.
\end{lemma}
\begin{proof} C-MWPC can be easily reduced to the MWPC problem assuming a
	coalescence graph without any edge or a fully connected interference graph.
	Therefore, each C-node is an uncoalesced live range after value separation
	and C-PC is equivalent to PC. A fully connected interference graph is made
	possible when all live ranges interfere with each other. Thus, the C-MWPC
	problem is NP-complete.
\end{proof}

\begin{lemma}[Lemma Subhead]The solution to the C-MWPC problem is no
	worse than the solution to the MWPC.
\end{lemma}
\begin{proof}
	Simply, any solution to the MWPC is also a solution to the
	C-MWPC. But some solutions to C-MWPC may not apply to the MWPC (if any
	coalescing were made).
\end{proof}

\section{Performance Evaluation}

During all the experiments, the Geographic Forwarding (GF)
\cite{Akyildiz-01} routing protocol is used. GF exploits geographic
information of nodes and conducts local data-forwarding to achieve
end-to-end routing. Our simulation is configured according to the
settings in Table~\ref{tab:one}. Each run lasts for 2 minutes and
repeated 100 times. For each data value we present in the results, we
also give its 90\% confidence interval.

% Table
\begin{table}%
	\caption{Simulation Configuration}
	\label{tab:one}
	\begin{minipage}{\columnwidth}
		\begin{center}
			\begin{tabular}{ll}
				\toprule
				TERRAIN\footnote{This is a table footnote. This is a
					table footnote. This is a table footnote.}   & (200m$\times$200m) Square\\
				Node Number     & 289\\
				Node Placement  & Uniform\\
				Application     & Many-to-Many/Gossip CBR Streams\\
				Payload Size    & 32 bytes\\
				Routing Layer   & GF\\
				MAC Layer       & CSMA/MMSN\\
				Radio Layer     & RADIO-ACCNOISE\\
				Radio Bandwidth & 250Kbps\\
				Radio Range     & 20m--45m\\
				\bottomrule
			\end{tabular}
		\end{center}
		\bigskip\centering
		\footnotesize\emph{Source:} This is a table
		sourcenote. This is a table sourcenote. This is a table
		sourcenote.

		\emph{Note:} This is a table footnote.
	\end{minipage}
\end{table}%


\section{Conclusions}

In this article, we develop the first multifrequency MAC protocol for
WSN applications in which each device adopts a
single radio transceiver. The different MAC design requirements for
WSNs and general wireless ad-hoc networks are
compared, and a complete WSN multifrequency MAC design (MMSN) is
put forth. During the MMSN design, we analyze and evaluate different
choices for frequency assignments and also discuss the nonuniform
back-off algorithms for the slotted media access design.

% Start of "Sample References" section

\section{Typical references in new ACM Reference Format}

To change from the current author-year citation style to a numeric citation style, comment out the line \verb|\setcitestyle{authoryear}| at the top of this file and instead uncomment the line \verb|\setcitestyle{acmnumeric}|. However, we recommend using the author-year citation style. In either citation style, to create citations that do not interrupt the sentence structure like~\cite{Abril07} use \verb|\cite| or \verb|\citep|, and to use citations that include the author names as part of the sentence like \citet{Abril07}, use \verb|\citet|.

Here are some sample references to various types of material: a paginated journal article \cite{Abril07}, an enumerated
journal article \cite{Cohen07}, a reference to an entire issue \cite{JCohen96},
a monograph (whole book) \cite{Kosiur01}, a monograph/whole book in a series (see 2a in spec. document)
\cite{Harel79}, a divisible-book such as an anthology or compilation \cite{Editor00}
followed by the same example, however we only output the series if the volume number is given
\cite{Editor00a} (so Editor00a's series should NOT be present since it has no vol. no.),
a chapter in a divisible book \cite{Spector90}, a chapter in a divisible book
in a series \cite{Douglass98}, a multi-volume work as book \cite{Knuth97},
an article in a proceedings (of a conference, symposium, workshop for example)
(paginated proceedings article) \cite{Andler79}, a proceedings article
with all possible elements \cite{Smith10}, an example of an enumerated
proceedings article \cite{VanGundy07},
an informally published work \cite{Harel78}, a doctoral dissertation \cite{Clarkson85},
a master's thesis: \cite{anisi03}, an online document / world wide web
resource \cite{Thornburg01, Ablamowicz07, Poker06}, a video game (Case 1) \cite{Obama08} and (Case 2) \cite{Novak03}
and \cite{Lee05} and (Case 3) a patent \cite{JoeScientist001},
work accepted for publication \cite{rous08}, 'YYYYb'-test for prolific author
\cite{SaeediMEJ10} and \cite{SaeediJETC10}. Other cites might contain
'duplicate' DOI and URLs (some SIAM articles) \cite{Kirschmer:2010:AEI:1958016.1958018}.
Boris / Barbara Beeton: multi-volume works as books
\cite{MR781536} and \cite{MR781537}.

% In the interest of anonymization, please do not include acknowledgements in your submission.
%
%\begin{acks}
%
%	The authors would like to thank Dr. Maura Turolla of Telecom
%	Italia for providing specifications about the application scenario.
%
%	The work is supported by the \grantsponsor{GS501100001809}{National
%		Natural Science Foundation of
%		China}{http://dx.doi.org/10.13039/501100001809} under Grant
%	No.:~\grantnum{GS501100001809}{61273304\_a}
%	and~\grantnum[http://www.nnsf.cn/youngscientsts]{GS501100001809}{Young
%		Scientsts' Support Program}.
%
%
%\end{acks}

% Bibliography
\bibliographystyle{ACM-Reference-Format}
\bibliography{sample-bibliography}

% Appendix
\appendix
\section{Switching times}

In this appendix, we measure the channel switching time of Micaz
\cite{CROSSBOW} sensor devices.  In our experiments, one mote
alternatingly switches between Channels~11 and~12. Every time after
the node switches to a channel, it sends out a packet immediately and
then changes to a new channel as soon as the transmission is finished.
We measure the number of packets the test mote can send in 10 seconds,
denoted as $N_{1}$. In contrast, we also measure the same value of the
test mote without switching channels, denoted as $N_{2}$. We calculate
the channel-switching time $s$ as
\begin{displaymath}%
s=\frac{10}{N_{1}}-\frac{10}{N_{2}}.
\end{displaymath}%
By repeating the experiments 100 times, we get the average
channel-switching time of Micaz motes: 24.3\,$\mu$s.

\section{Supplementary materials}

	\subsection{This is an example of Appendix subsection head}

	Channel-switching time is measured as the time length it takes for
	motes to successfully switch from one channel to another. This
	parameter impacts the maximum network throughput, because motes
	cannot receive or send any packet during this period of time, and it
	also affects the efficiency of toggle snooping in MMSN, where motes
	need to sense through channels rapidly.

	By repeating experiments 100 times, we get the average
	channel-switching time of Micaz motes: 24.3 $\mu$s. We then conduct
	the same experiments with different Micaz motes, as well as
	experiments with the transmitter switching from Channel 11 to other
	channels. In both scenarios, the channel-switching time does not have
	obvious changes. (In our experiments, all values are in the range of
	23.6 $\mu$s to 24.9 $\mu$s.)

	\subsection{Appendix subsection head}

	The primary consumer of energy in WSNs is idle listening. The key to
	reduce idle listening is executing low duty-cycle on nodes. Two
	primary approaches are considered in controlling duty-cycles in the
	MAC layer.

\end{document}
